{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["塑料管"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"塑料管","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"merged":[[0,0,0,1],[1,0,1,6],[3,3,10,3],[15,3,19,3],[27,3,28,3],[40,0,40,6],[41,0,41,5],[42,0,42,5],[43,0,43,5],[44,0,44,5],[45,0,45,5]],"flags":["formulas_cached_only"]}
["附件"]
["惠州市江北污水处理厂二期工程项目施工管材采购项目询价报价表"]
["序号","材料名称","规格型号或指标","技术参数","单位","报价（元）","备注"]
[1,"PE给水管","DN500，PN=1.0MPa","1.管道压力等级1.0MPa；\n2.管材应符合《给水用聚乙烯（PE）管道系统 第2部分：管材》（GB/T 13663.2-2018）要求；\n3.给水管道连接采用热熔粘接和法兰连接。","m"]
[2,"PE给水管","DN150，PN=1.0MPa",null,"m"]
[3,"PE给水管","DN100，PN=1.0MPa",null,"m"]
[4,"PE给水管","DN80，PN=1.0MPa",null,"m"]
[5,"PE给水管","DN50，PN=1.0MPa",null,"m"]
[6,"PE给水管","DN25，PN=1.0MPa",null,"m"]
[7,"PE给水管","DN20，PN=1.0MPa",null,"m"]
[8,"PE给水管","De400",null,"m"]
[9,"UPVC塑料管","DN50",null,"m"]
[10,"UPVC排水管","DN25",null,"m"]
[11,"UPVC管","DN25",null,"m"]
[12,"UPVC管","DN32",null,"m"]
[13,"UPVC给水管","De63，PN=1.0MPa","1.管道压力等级1.0MPa；\n2.管材应符合《给水用聚乙烯（PE）管道系统 第2部分：管材》（GB/T 13663.2-2018）要求；\n3.给水管道连接采用热熔粘接和法兰连接。","m"]
[14,"UPVC给水管","De32，PN=1.0MPa",null,"m"]
[15,"UPVC给水管","De110，PN=1.0MPa",null,"m"]
[16,"UPVC给水管","De50，PN=1.0MPa",null,"m"]
[17,"UPVC给水管","De20，PN=1.0MPa",null,"m"]
[18,"PVC塑料排水管","DN50",null,"m"]
[19,"塑料排水管","DN25",null,"m"]
[20,"塑料排水管","DN75",null,"m"]
[21,"塑料排水管","DN150",null,"m"]
[22,"塑料软管","D5",null,"m"]
[23,"塑料软管","D9",null,"m"]
[24,"塑料软管","D20",null,"m"]
[25,"Ⅲ级钢筋混凝土管","D1400","选用《混凝土和钢筋混凝土排水管》(GB/T 11836-2023)中顶进施工用钢筋混凝土管DRCPⅢ400x2500 GB/T 11836；接口连接方式:柔性接口钢承口管，采用“A” 型连接。管道接口:采用楔形橡胶密封圈柔性接口。橡胶圈材料,采用氯丁橡胶。","m"]
[26,"Ⅲ级钢筋砼管","D1000",null,"m"]
[27,"II级钢筋混凝土管","d600","承插式橡胶圈接口；承压能力应不小于0.3MPa","m"]
[28,"II级钢筋混凝土管","d300","承插式橡胶圈接口；承压能力应不小于0.3MPa","m"]
[29,"II级钢筋混凝土管","d400","承插式橡胶圈接口；承压能力应不小于0.3MPa","m"]
[30,"II级钢筋混凝土管","d2000","承插式橡胶圈接口；承压能力应不小于0.3MPa","m"]
[31,"II级钢筋混凝土管","d500","承插式橡胶圈接口；承压能力应不小于0.3MPa","m"]
[32,"夹砂玻璃钢管","DN1600","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用承插接口","m"]
[33,"夹砂玻璃钢管","DN1000","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用承插接口","m"]
[34,"夹砂玻璃钢管","DN600","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用承插接口","m"]
[35,"夹砂玻璃钢管","DN400","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用包缠粘接","m"]
[36,"夹砂玻璃钢管","DN300","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用包缠粘接","m"]
[37,"夹砂玻璃钢管","DN200","环刚度为SN10(KPa)；压力等级为1.0Mpa；采用包缠粘接","m"]
["注：单价包含材料费（包含配套材料、辅助材料等，如钢管现场焊接施工所需的防腐材料）、人工费、机械费、制作费、试验检测费、包装费、运杂费（包括装卸车费）、培训费、保险费、缺陷修复费、综合管理费、技术资料费、风险费、利润、各种税费、政策性文件规定费用等一切费用，即货物到达交货地点所发生的一切费用；数量以采购人实际采购数量为准，送货量月结80%，当年结算至97%，质量保证金3%完工一年后付清，具体以签订的合同条款为准。"]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话："]
["日    期："]